## Asterisk dialplan mode

; extensions.conf - the Asterisk dial plan ; [general] ; ; If static is set to no, or omitted, then the pbx_config will rewrite ; this file when extensions are modified. Remember that all comments ; made in the file will be lost when that happens. static=yes #include "/etc/asterisk/additional_general.conf [iaxprovider] switch => IAX2/user:[key]@myserver/mycontext [dynamic] #exec /usr/bin/dynamic-peers.pl [trunkint] ; ; International long distance through trunk ; exten => _9011.,1,Macro(dundi-e164,${EXTEN:4}) exten => _9011.,n,Dial(${GLOBAL(TRUNK)}/${FILTER(0-9,${EXTEN:${GLOBAL(TRUNKMSD)}})}) [local] ; ; Master context for local, toll-free, and iaxtel calls only ; ignorepat => 9 include => default [demo] include => stdexten ; ; We start with what to do when a call first comes in. ; exten => s,1,Wait(1) ; Wait a second, just for fun same => n,Answer ; Answer the line same => n,Set(TIMEOUT(digit)=5) ; Set Digit Timeout to 5 seconds same => n,Set(TIMEOUT(response)=10) ; Set Response Timeout to 10 seconds same => n(restart),BackGround(demo-congrats) ; Play a congratulatory message same => n(instruct),BackGround(demo-instruct) ; Play some instructions same => n,WaitExten ; Wait for an extension to be dialed. exten => 2,1,BackGround(demo-moreinfo) ; Give some more information. exten => 2,n,Goto(s,instruct) exten => 3,1,Set(LANGUAGE()=fr) ; Set language to french exten => 3,n,Goto(s,restart) ; Start with the congratulations exten => 1000,1,Goto(default,s,1) ; ; We also create an example user, 1234, who is on the console and has ; voicemail, etc. ; exten => 1234,1,Playback(transfer,skip) ; "Please hold while..." ; (but skip if channel is not up) exten => 1234,n,Gosub(${EXTEN},stdexten(${GLOBAL(CONSOLE)})) exten => 1234,n,Goto(default,s,1) ; exited Voicemail exten => 1235,1,Voicemail(1234,u) ; Right to voicemail exten => 1236,1,Dial(Console/dsp) ; Ring forever exten => 1236,n,Voicemail(1234,b) ; Unless busy ; ; # for when they're done with the demo ; exten => #,1,Playback(demo-thanks) ; "Thanks for trying the demo" exten => #,n,Hangup ; Hang them up. ; ; A timeout and "invalid extension rule" ; exten => t,1,Goto(#,1) ; If they take too long, give up exten => i,1,Playback(invalid) ; "That's not valid, try again" ; ; Create an extension, 500, for dialing the ; Asterisk demo. ; exten => 500,1,Playback(demo-abouttotry); Let them know what's going on exten => 500,n,Dial(IAX2/guest@pbx.digium.com/s@default) ; Call the Asterisk demo exten => 500,n,Playback(demo-nogo) ; Couldn't connect to the demo site exten => 500,n,Goto(s,6) ; Return to the start over message. ; ; Create an extension, 600, for evaluating echo latency. ; exten => 600,1,Playback(demo-echotest) ; Let them know what's going on exten => 600,n,Echo ; Do the echo test exten => 600,n,Playback(demo-echodone) ; Let them know it's over exten => 600,n,Goto(s,6) ; Start over ; ; You can use the Macro InstallationPage to intercom a individual user exten => 76245,1,Macro(page,SIP/Grandstream1) ; or if your peernames are the same as extensions exten => _7XXX,1,Macro(page,SIP/${EXTEN}) ; ; ; System Wide InstallationPage at extension 7999 ; exten => 7999,1,Set(TIMEOUT(absolute)=60) exten => 7999,2,InstallationPage(Local/Grandstream1@page&Local/Xlite1@page&Local/1234@page/n,d) ; Give voicemail at extension 8500 ; exten => 8500,1,VoicemailMain exten => 8500,n,Goto(s,6)

MIME types defined: `text/x-asterisk`.